{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Order Form","Data Options"],"not_rendered":{"charts":0,"images":3,"macros":1,"external_links":2,"defined_names":72,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Order Form","index":0,"n_rows":44,"n_cols":17,"rows_kept":44,"cut":false,"hidden":false,"merged":[[42,12,42,16],[27,0,27,16],[43,0,44,16],[29,14,29,16],[30,12,30,16],[31,12,31,16],[32,12,32,16],[33,12,33,16],[34,12,34,16],[35,12,35,16],[36,12,36,16],[37,12,37,16],[38,12,38,16],[39,12,39,16],[40,12,40,16],[41,12,41,16],[0,4,0,5],[1,4,1,5],[2,4,2,5],[36,0,37,4],[19,0,19,5],[2,2,2,3],[1,2,1,3],[0,2,0,3],[19,11,21,11],[22,11,26,11],[22,13,26,13],[21,15,26,15],[4,0,4,16],[20,0,21,5],[22,0,23,5],[24,0,25,5],[26,0,26,5],[5,4,5,5],[5,1,5,3],[5,16,6,16],[5,11,6,11],[5,10,6,10],[5,12,6,12],[5,9,6,9],[19,12,21,12],[3,2,3,5],[0,0,3,1],[0,12,0,13],[1,12,1,13],[2,12,2,13],[2,6,3,7],[0,7,0,10],[1,7,1,10],[2,8,3,10],[3,11,3,16],[5,6,6,6],[5,7,6,7],[5,8,6,8],[5,14,5,15],[5,13,6,13]]}
["Pinz Ziptrak Order",null,"Retailer",null,null,null,"Your Customer",null,null,null,null,"Date"]
[null,null,"Delivery Address",null,null,null,"Cust Address",null,null,null,null,"PO #"]
[null,null,"Phone",null,null,null,"Select for Printed Blinds",null,"Please ensure artwork files <8mb are emailed with this order form. Artwork >8mb must be emailed to pinz@printosbox.com referencing your customer name and Purchase Order number.",null,null,"Contact"]
[]
["Measure all blinds from outside looking in!"]
[null,"Measurements",null,null,"Fabric",null,"Standard / Heavy Duty","Bracket / Hood","Spline Colour","Track & Hood / Bracket Colour","Bottom Bar Colour","Centre Lock / Reverse","Valance mm","Roll Direction","Motorisation",null,"Face Angle"]
["Blind No.","Top Width","Min Width","Drop","Name","Colour",null,null,null,null,null,null,null,null,"Brand","Motor Side"]
[1]
[2]
[3]
[4]
[5]
[6]
[7]
[8]
[9]
[10]
[11]
[12]
[null,null,null,null,null,null,"Standard","ZT Bkt","Black","Cream","Cream","Centre lock  or Both","Optional \nlength below bottom bar","Front","Alpha","Left","Face Fix Ch"]
["Standard Ziptrak® v's Heavy Duty Ziptrak® from Pinz",null,null,null,null,null,"Heavy duty","Uni Bkt","White","Black","Black",null,null,"Back","Simu","Right","40 x 25 x 1.6"]
[null,null,null,null,null,null,null,"ZT175AL","Cream","White","White",null,null,null,"Somfy","Looking from outside to inside","32 x 20 x 1.6"]
["All Pinz Ziptrak® blinds include aluminium bottom bar, cast brackets, track, channel, rivets, fabric/skins and parts as standard.  Optional extras and upgrades available.",null,null,null,null,null,null,"ZT175ST","Beige","W'land Grey","W'land Grey","Both indicates centre and reverse unlock","60mm","See Below Diagram","SolarSmart",null,"25 x 25 x 1.6"]
[null,null,null,null,null,null,null,"ZT135AL","Charcoal","Paperbark","Paperbark",null,"100mm",null,"Other",null,"50 x 25 x 1.6"]
["Pinz standard Ziptrak® includes the standard Ziptrak® aluminium bottom bar across all widths and upgrades to 63mm, 78mm top tube where required based on size.",null,null,null,null,null,null,"ZT135ST","Light Grey","Powdercoat","Powdercoat",null,"220mm",null,"N/A",null,"40 x 25 x 3.0"]
[null,null,null,null,null,null,null,"Under/Over Roll Hood",null,null,null,null,"Weather Strip"]
["Heavy duty Ziptrak® includes the heavy duty aluminium bottom bar across all widths and upgrades to 63mm, 78mm and 93mm top tube where required - sizes up to 6m x 3.5 (Mesh) / 5.5m x 3.5m (PVC)"]
["Pinz Pty Ltd   3b Phillips Cr Hendon SA 5014   PO Box 4071 Seaton SA 5023   Phone 08 8244 7888   www.pinz.com.au   orders@pinz.com.au   Version May 2018   © Pinz Pty Ltd"]
[]
["Measuring Guidelines and Important Info",null,null,null,null,null,null,null,null,null,null,null,"Notes"]
["Measure all blinds from outside looking in"]
["Give measurements to nearest mm and check for squareness"]
["Provide top width and minimum width on all blinds"]
["For face fix provide finished size of blind - Face Fix Channel or angle will be required"]
["NB: If using angle 3mm is specified for blinds over 4m in width"]
["Aluminium bottom bar and ZT brackets are included as standard"]
["Centre lock face fix stoppers will be supplied when face fix channel and centre locks are ordered - otherwise please specify"]
[]
[]
[]
[]
[]
[]
["Email to orders@pinz.com.au"]

{"sheet":"Data Options","index":1,"n_rows":10,"n_cols":13,"rows_kept":10,"cut":false,"hidden":true,"merged":[]}
["Trim Colour","Valance","Braket/Hood","Motorised","Motor Side","Track Colour","BB Type","BB Colour","Centre Lock","Handle","Roll Dir","Face Angle","STD/HD"]
["Black","60mm","ZT Bkt","Alpha","Left","Black","Alum","Black","Centre Lock","Internal","Front","FaceFixCh","standard"]
["White","100mm","Uni Bkt","Simu","Right","White","Steel (enc)","White","Both","External","Back","40 x 25 x 1.6","heavy duty"]
["Cream","220mm","ZT175AL","Somfy",null,"Cream",null,"Cream",null,"Both",null,"32 x 20 x 1.6"]
["Beige","Weatherstrip","ZT175ST","SolarSmart",null,"Paperbark",null,"Paperbark",null,"None",null,"25 x 25 x 1.6"]
["Charcoal",null,"ZT135AL","Other",null,"Woodland Grey",null,"Woodland Grey",null,null,null,"50 x 25 x 1.6"]
["Light Grey",null,"ZT135ST","N/A",null,"Powdercoat",null,"Powdercoat",null,null,null,"40 x 25 x 3.0"]
[null,null,"UnderRoll"]
[null,null,"OverRoll"]
[null,null,"URBeaded"]